


Thermal Couple Measurement on 1218


Based on TC1 (average: roughly: 35.5 degC)



TC TC1

After shifting: make the value measured at (304,297) close to 35.5degC 🡪 deduct 12 degC from all values in the image TC1










(c)


(a)


(d)



(b)



Based on TC3 (average: roughly: 33.52 degC)



 TC3

After shifting: make the value measured at (250,294) close to 33.52degC 🡪 deduct 13.5 degC from all values in the image TC3

(c)

(a)

(d)

(b)

